# Changelog
All notable changes to this project will be documented in this file.

The format is based on [Keep a Changelog](https://keepachangelog.com/en/1.0.0/),
and this project adheres to [Semantic Versioning](https://semver.org/spec/v2.0.0.html).

## [Unreleased]

## [1.4] - 2026-05-22
### Added
* Support new models:
  - DA-920E
  - V2202D
  - V2406D
  - BXP-C101
  - BXP-C200
  - DRP-C200
  - MPC-3001
  - DRP-C200
* Add source list:
  - Driver:
    + 'ast-drm-driver' version 1.15.3-moxa1
    + 'siliconmotion-smifb-driver' version 4.6.0
    + 'moxa-ltc3350-driver' version 1.3.0
    + 'moxa-it87-driver' version 6.12
    + 'moxa-gpio-pca953x-driver' version 6.12
    + 'moxa-mxuport-driver' version 5.3.5
    + 'moxa-mxuport-driver' version 6.2.5-1
  - Tools:
    + 'moxa-x86-control-tools' version 2.23.0, 2.26.0, 2.27.0, 2.28.0 and 2.30.0
    + 'moxa-mcu-manager' version 1.3.0
    + 'moxa-power-manager' version 2.2.3
* Add packages list:
  - 'Moxa Connection Manager' version 1.7.18-1ubuntu1

### Changed
* Update BXP-A100/BXP-C100 model:
  - Update 'Moxa Connection Manager' version to 1.7.17-1ubuntu1
  - Update 'moxa-x86-control-tools' version to 2.23.0

### Fixed
* Handle compressed kernel modules (zst/xz) installation/uninstallation correctly
* libgpiod self-test shall check /usr/local/bin is exist on env PATH
* moxa-x86-control-tools self-test shall check mx-usb-power-ctl is installed
* moxa-x86-control-tools self-test count valid serialport until return error
* Correct moxa-mcu-manager self-test output alignment
